[0.000000] (-) TimerEvent: {}
[0.000214] (arduino_bridge) JobQueued: {'identifier': 'arduino_bridge', 'dependencies': OrderedDict()}
[0.000312] (arduino_bridge_cpp) JobQueued: {'identifier': 'arduino_bridge_cpp', 'dependencies': OrderedDict()}
[0.001822] (arduino_bridge) JobStarted: {'identifier': 'arduino_bridge'}
[0.021493] (arduino_bridge_cpp) JobStarted: {'identifier': 'arduino_bridge_cpp'}
[0.099682] (-) TimerEvent: {}
[0.200061] (-) TimerEvent: {}
[0.300461] (-) TimerEvent: {}
[0.400990] (-) TimerEvent: {}
[0.495409] (arduino_bridge_cpp) JobProgress: {'identifier': 'arduino_bridge_cpp', 'progress': 'cmake'}
[0.496660] (arduino_bridge_cpp) JobProgress: {'identifier': 'arduino_bridge_cpp', 'progress': 'build'}
[0.498265] (arduino_bridge_cpp) Command: {'cmd': ['/usr/bin/cmake', '--build', '/home/koray/ros2_ws/build/arduino_bridge_cpp', '--', '-j4', '-l4'], 'cwd': '/home/koray/ros2_ws/build/arduino_bridge_cpp', 'env': OrderedDict([('LESSOPEN', '| /usr/bin/lesspipe %s'), ('MESA_LOADER_DRIVER_OVERRIDE', 'iris'), ('HOSTNAME', 'a1c8d42d73da'), ('SHLVL', '1'), ('LD_LIBRARY_PATH', '/opt/ros/humble/opt/rviz_ogre_vendor/lib:/opt/ros/humble/lib/x86_64-linux-gnu:/opt/ros/humble/lib'), ('HOME', '/home/koray'), ('CYCLONEDDS_URI', 'file:///etc/cyclonedds/config.xml'), ('ROS_PYTHON_VERSION', '3'), ('ROS_DISTRO', 'humble'), ('_', '/usr/bin/colcon'), ('ROS_VERSION', '2'), ('TERM', 'xterm'), ('ROS_LOCALHOST_ONLY', '0'), ('PATH', '/opt/ros/humble/bin:/usr/local/sbin:/usr/local/bin:/usr/sbin:/usr/bin:/sbin:/bin'), ('DISPLAY', ':0'), ('LANG', 'C.UTF-8'), ('RMW_IMPLEMENTATION', 'rmw_cyclonedds_cpp'), ('LIBVA_DRIVER_NAME', 'i965'), ('LS_COLORS', 'rs=0:di=01;34:ln=01;36:mh=00:pi=40;33:so=01;35:do=01;35:bd=40;33;01:cd=40;33;01:or=40;31;01:mi=00:su=37;41:sg=30;43:ca=30;41:tw=30;42:ow=34;42:st=37;44:ex=01;32:*.tar=01;31:*.tgz=01;31:*.arc=01;31:*.arj=01;31:*.taz=01;31:*.lha=01;31:*.lz4=01;31:*.lzh=01;31:*.lzma=01;31:*.tlz=01;31:*.txz=01;31:*.tzo=01;31:*.t7z=01;31:*.zip=01;31:*.z=01;31:*.dz=01;31:*.gz=01;31:*.lrz=01;31:*.lz=01;31:*.lzo=01;31:*.xz=01;31:*.zst=01;31:*.tzst=01;31:*.bz2=01;31:*.bz=01;31:*.tbz=01;31:*.tbz2=01;31:*.tz=01;31:*.deb=01;31:*.rpm=01;31:*.jar=01;31:*.war=01;31:*.ear=01;31:*.sar=01;31:*.rar=01;31:*.alz=01;31:*.ace=01;31:*.zoo=01;31:*.cpio=01;31:*.7z=01;31:*.rz=01;31:*.cab=01;31:*.wim=01;31:*.swm=01;31:*.dwm=01;31:*.esd=01;31:*.jpg=01;35:*.jpeg=01;35:*.mjpg=01;35:*.mjpeg=01;35:*.gif=01;35:*.bmp=01;35:*.pbm=01;35:*.pgm=01;35:*.ppm=01;35:*.tga=01;35:*.xbm=01;35:*.xpm=01;35:*.tif=01;35:*.tiff=01;35:*.png=01;35:*.svg=01;35:*.svgz=01;35:*.mng=01;35:*.pcx=01;35:*.mov=01;35:*.mpg=01;35:*.mpeg=01;35:*.m2v=01;35:*.mkv=01;35:*.webm=01;35:*.webp=01;35:*.ogm=01;35:*.mp4=01;35:*.m4v=01;35:*.mp4v=01;35:*.vob=01;35:*.qt=01;35:*.nuv=01;35:*.wmv=01;35:*.asf=01;35:*.rm=01;35:*.rmvb=01;35:*.flc=01;35:*.avi=01;35:*.fli=01;35:*.flv=01;35:*.gl=01;35:*.dl=01;35:*.xcf=01;35:*.xwd=01;35:*.yuv=01;35:*.cgm=01;35:*.emf=01;35:*.ogv=01;35:*.ogx=01;35:*.aac=00;36:*.au=00;36:*.flac=00;36:*.m4a=00;36:*.mid=00;36:*.midi=00;36:*.mka=00;36:*.mp3=00;36:*.mpc=00;36:*.ogg=00;36:*.ra=00;36:*.wav=00;36:*.oga=00;36:*.opus=00;36:*.spx=00;36:*.xspf=00;36:'), ('AMENT_PREFIX_PATH', '/opt/ros/humble'), ('DEBIAN_FRONTEND', 'noninteractive'), ('SHELL', '/bin/bash'), ('LESSCLOSE', '/usr/bin/lesspipe %s %s'), ('PWD', '/home/koray/ros2_ws/build/arduino_bridge_cpp'), ('QT_QPA_PLATFORM', 'xcb'), ('LC_ALL', 'C.UTF-8'), ('PYTHONPATH', '/opt/ros/humble/lib/python3.10/site-packages:/opt/ros/humble/local/lib/python3.10/dist-packages'), ('COLCON', '1'), ('CMAKE_PREFIX_PATH', '/opt/ros/humble')]), 'shell': False}
[0.501064] (-) TimerEvent: {}
[0.604726] (-) TimerEvent: {}
[0.645161] (arduino_bridge_cpp) StdoutLine: {'line': b'[100%] Built target arduino_bridge\n'}
[0.668648] (arduino_bridge_cpp) CommandEnded: {'returncode': 0}
[0.669977] (arduino_bridge_cpp) JobProgress: {'identifier': 'arduino_bridge_cpp', 'progress': 'install'}
[0.687001] (arduino_bridge_cpp) Command: {'cmd': ['/usr/bin/cmake', '--install', '/home/koray/ros2_ws/build/arduino_bridge_cpp'], 'cwd': '/home/koray/ros2_ws/build/arduino_bridge_cpp', 'env': OrderedDict([('LESSOPEN', '| /usr/bin/lesspipe %s'), ('MESA_LOADER_DRIVER_OVERRIDE', 'iris'), ('HOSTNAME', 'a1c8d42d73da'), ('SHLVL', '1'), ('LD_LIBRARY_PATH', '/opt/ros/humble/opt/rviz_ogre_vendor/lib:/opt/ros/humble/lib/x86_64-linux-gnu:/opt/ros/humble/lib'), ('HOME', '/home/koray'), ('CYCLONEDDS_URI', 'file:///etc/cyclonedds/config.xml'), ('ROS_PYTHON_VERSION', '3'), ('ROS_DISTRO', 'humble'), ('_', '/usr/bin/colcon'), ('ROS_VERSION', '2'), ('TERM', 'xterm'), ('ROS_LOCALHOST_ONLY', '0'), ('PATH', '/opt/ros/humble/bin:/usr/local/sbin:/usr/local/bin:/usr/sbin:/usr/bin:/sbin:/bin'), ('DISPLAY', ':0'), ('LANG', 'C.UTF-8'), ('RMW_IMPLEMENTATION', 'rmw_cyclonedds_cpp'), ('LIBVA_DRIVER_NAME', 'i965'), ('LS_COLORS', 'rs=0:di=01;34:ln=01;36:mh=00:pi=40;33:so=01;35:do=01;35:bd=40;33;01:cd=40;33;01:or=40;31;01:mi=00:su=37;41:sg=30;43:ca=30;41:tw=30;42:ow=34;42:st=37;44:ex=01;32:*.tar=01;31:*.tgz=01;31:*.arc=01;31:*.arj=01;31:*.taz=01;31:*.lha=01;31:*.lz4=01;31:*.lzh=01;31:*.lzma=01;31:*.tlz=01;31:*.txz=01;31:*.tzo=01;31:*.t7z=01;31:*.zip=01;31:*.z=01;31:*.dz=01;31:*.gz=01;31:*.lrz=01;31:*.lz=01;31:*.lzo=01;31:*.xz=01;31:*.zst=01;31:*.tzst=01;31:*.bz2=01;31:*.bz=01;31:*.tbz=01;31:*.tbz2=01;31:*.tz=01;31:*.deb=01;31:*.rpm=01;31:*.jar=01;31:*.war=01;31:*.ear=01;31:*.sar=01;31:*.rar=01;31:*.alz=01;31:*.ace=01;31:*.zoo=01;31:*.cpio=01;31:*.7z=01;31:*.rz=01;31:*.cab=01;31:*.wim=01;31:*.swm=01;31:*.dwm=01;31:*.esd=01;31:*.jpg=01;35:*.jpeg=01;35:*.mjpg=01;35:*.mjpeg=01;35:*.gif=01;35:*.bmp=01;35:*.pbm=01;35:*.pgm=01;35:*.ppm=01;35:*.tga=01;35:*.xbm=01;35:*.xpm=01;35:*.tif=01;35:*.tiff=01;35:*.png=01;35:*.svg=01;35:*.svgz=01;35:*.mng=01;35:*.pcx=01;35:*.mov=01;35:*.mpg=01;35:*.mpeg=01;35:*.m2v=01;35:*.mkv=01;35:*.webm=01;35:*.webp=01;35:*.ogm=01;35:*.mp4=01;35:*.m4v=01;35:*.mp4v=01;35:*.vob=01;35:*.qt=01;35:*.nuv=01;35:*.wmv=01;35:*.asf=01;35:*.rm=01;35:*.rmvb=01;35:*.flc=01;35:*.avi=01;35:*.fli=01;35:*.flv=01;35:*.gl=01;35:*.dl=01;35:*.xcf=01;35:*.xwd=01;35:*.yuv=01;35:*.cgm=01;35:*.emf=01;35:*.ogv=01;35:*.ogx=01;35:*.aac=00;36:*.au=00;36:*.flac=00;36:*.m4a=00;36:*.mid=00;36:*.midi=00;36:*.mka=00;36:*.mp3=00;36:*.mpc=00;36:*.ogg=00;36:*.ra=00;36:*.wav=00;36:*.oga=00;36:*.opus=00;36:*.spx=00;36:*.xspf=00;36:'), ('AMENT_PREFIX_PATH', '/opt/ros/humble'), ('DEBIAN_FRONTEND', 'noninteractive'), ('SHELL', '/bin/bash'), ('LESSCLOSE', '/usr/bin/lesspipe %s %s'), ('PWD', '/home/koray/ros2_ws/build/arduino_bridge_cpp'), ('QT_QPA_PLATFORM', 'xcb'), ('LC_ALL', 'C.UTF-8'), ('PYTHONPATH', '/opt/ros/humble/lib/python3.10/site-packages:/opt/ros/humble/local/lib/python3.10/dist-packages'), ('COLCON', '1'), ('CMAKE_PREFIX_PATH', '/opt/ros/humble')]), 'shell': False}
[0.703607] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Install configuration: ""\n'}
[0.704408] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/lib/arduino_bridge_cpp/arduino_bridge\n'}
[0.704776] (-) TimerEvent: {}
[0.705376] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/ament_index/resource_index/package_run_dependencies/arduino_bridge_cpp\n'}
[0.706503] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/ament_index/resource_index/parent_prefix_path/arduino_bridge_cpp\n'}
[0.706960] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/environment/ament_prefix_path.sh\n'}
[0.707196] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/environment/ament_prefix_path.dsv\n'}
[0.707412] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/environment/path.sh\n'}
[0.707663] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/environment/path.dsv\n'}
[0.708082] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/local_setup.bash\n'}
[0.708329] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/local_setup.sh\n'}
[0.708563] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/local_setup.zsh\n'}
[0.709436] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/local_setup.dsv\n'}
[0.709720] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Installing: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/package.dsv\n'}
[0.709954] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/ament_index/resource_index/packages/arduino_bridge_cpp\n'}
[0.710180] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/cmake/arduino_bridge_cppConfig.cmake\n'}
[0.710392] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/cmake/arduino_bridge_cppConfig-version.cmake\n'}
[0.710595] (arduino_bridge_cpp) StdoutLine: {'line': b'-- Up-to-date: /home/koray/ros2_ws/install/arduino_bridge_cpp/share/arduino_bridge_cpp/package.xml\n'}
[0.713482] (arduino_bridge_cpp) CommandEnded: {'returncode': 0}
[0.748462] (arduino_bridge_cpp) JobEnded: {'identifier': 'arduino_bridge_cpp', 'rc': 0}
[0.804930] (-) TimerEvent: {}
[0.905265] (-) TimerEvent: {}
[1.005589] (-) TimerEvent: {}
[1.105931] (-) TimerEvent: {}
[1.150072] (arduino_bridge) Command: {'cmd': ['/usr/bin/python3', '-W', 'ignore:setup.py install is deprecated', '-W', 'ignore:easy_install command is deprecated', 'setup.py', 'egg_info', '--egg-base', '../../build/arduino_bridge', 'build', '--build-base', '/home/koray/ros2_ws/build/arduino_bridge/build', 'install', '--record', '/home/koray/ros2_ws/build/arduino_bridge/install.log', '--single-version-externally-managed', 'install_data'], 'cwd': '/home/koray/ros2_ws/src/arduino_bridge', 'env': {'LESSOPEN': '| /usr/bin/lesspipe %s', 'MESA_LOADER_DRIVER_OVERRIDE': 'iris', 'HOSTNAME': 'a1c8d42d73da', 'SHLVL': '1', 'LD_LIBRARY_PATH': '/opt/ros/humble/opt/rviz_ogre_vendor/lib:/opt/ros/humble/lib/x86_64-linux-gnu:/opt/ros/humble/lib', 'HOME': '/home/koray', 'CYCLONEDDS_URI': 'file:///etc/cyclonedds/config.xml', 'ROS_PYTHON_VERSION': '3', 'ROS_DISTRO': 'humble', '_': '/usr/bin/colcon', 'ROS_VERSION': '2', 'TERM': 'xterm', 'ROS_LOCALHOST_ONLY': '0', 'PATH': '/opt/ros/humble/bin:/usr/local/sbin:/usr/local/bin:/usr/sbin:/usr/bin:/sbin:/bin', 'DISPLAY': ':0', 'LANG': 'C.UTF-8', 'RMW_IMPLEMENTATION': 'rmw_cyclonedds_cpp', 'LIBVA_DRIVER_NAME': 'i965', 'LS_COLORS': 'rs=0:di=01;34:ln=01;36:mh=00:pi=40;33:so=01;35:do=01;35:bd=40;33;01:cd=40;33;01:or=40;31;01:mi=00:su=37;41:sg=30;43:ca=30;41:tw=30;42:ow=34;42:st=37;44:ex=01;32:*.tar=01;31:*.tgz=01;31:*.arc=01;31:*.arj=01;31:*.taz=01;31:*.lha=01;31:*.lz4=01;31:*.lzh=01;31:*.lzma=01;31:*.tlz=01;31:*.txz=01;31:*.tzo=01;31:*.t7z=01;31:*.zip=01;31:*.z=01;31:*.dz=01;31:*.gz=01;31:*.lrz=01;31:*.lz=01;31:*.lzo=01;31:*.xz=01;31:*.zst=01;31:*.tzst=01;31:*.bz2=01;31:*.bz=01;31:*.tbz=01;31:*.tbz2=01;31:*.tz=01;31:*.deb=01;31:*.rpm=01;31:*.jar=01;31:*.war=01;31:*.ear=01;31:*.sar=01;31:*.rar=01;31:*.alz=01;31:*.ace=01;31:*.zoo=01;31:*.cpio=01;31:*.7z=01;31:*.rz=01;31:*.cab=01;31:*.wim=01;31:*.swm=01;31:*.dwm=01;31:*.esd=01;31:*.jpg=01;35:*.jpeg=01;35:*.mjpg=01;35:*.mjpeg=01;35:*.gif=01;35:*.bmp=01;35:*.pbm=01;35:*.pgm=01;35:*.ppm=01;35:*.tga=01;35:*.xbm=01;35:*.xpm=01;35:*.tif=01;35:*.tiff=01;35:*.png=01;35:*.svg=01;35:*.svgz=01;35:*.mng=01;35:*.pcx=01;35:*.mov=01;35:*.mpg=01;35:*.mpeg=01;35:*.m2v=01;35:*.mkv=01;35:*.webm=01;35:*.webp=01;35:*.ogm=01;35:*.mp4=01;35:*.m4v=01;35:*.mp4v=01;35:*.vob=01;35:*.qt=01;35:*.nuv=01;35:*.wmv=01;35:*.asf=01;35:*.rm=01;35:*.rmvb=01;35:*.flc=01;35:*.avi=01;35:*.fli=01;35:*.flv=01;35:*.gl=01;35:*.dl=01;35:*.xcf=01;35:*.xwd=01;35:*.yuv=01;35:*.cgm=01;35:*.emf=01;35:*.ogv=01;35:*.ogx=01;35:*.aac=00;36:*.au=00;36:*.flac=00;36:*.m4a=00;36:*.mid=00;36:*.midi=00;36:*.mka=00;36:*.mp3=00;36:*.mpc=00;36:*.ogg=00;36:*.ra=00;36:*.wav=00;36:*.oga=00;36:*.opus=00;36:*.spx=00;36:*.xspf=00;36:', 'AMENT_PREFIX_PATH': '/opt/ros/humble', 'DEBIAN_FRONTEND': 'noninteractive', 'SHELL': '/bin/bash', 'LESSCLOSE': '/usr/bin/lesspipe %s %s', 'PWD': '/home/koray/ros2_ws/build/arduino_bridge', 'QT_QPA_PLATFORM': 'xcb', 'LC_ALL': 'C.UTF-8', 'PYTHONPATH': '/home/koray/ros2_ws/build/arduino_bridge/prefix_override:/usr/lib/python3/dist-packages/colcon_core/task/python/colcon_distutils_commands:/home/koray/ros2_ws/install/arduino_bridge/lib/python3.10/site-packages:/opt/ros/humble/lib/python3.10/site-packages:/opt/ros/humble/local/lib/python3.10/dist-packages', 'COLCON': '1'}, 'shell': False}
[1.206074] (-) TimerEvent: {}
[1.306453] (-) TimerEvent: {}
[1.406821] (-) TimerEvent: {}
[1.507176] (-) TimerEvent: {}
[1.554575] (arduino_bridge) StdoutLine: {'line': b'running egg_info\n'}
[1.555861] (arduino_bridge) StdoutLine: {'line': b'writing ../../build/arduino_bridge/arduino_bridge.egg-info/PKG-INFO\n'}
[1.556329] (arduino_bridge) StdoutLine: {'line': b'writing dependency_links to ../../build/arduino_bridge/arduino_bridge.egg-info/dependency_links.txt\n'}
[1.556638] (arduino_bridge) StdoutLine: {'line': b'writing entry points to ../../build/arduino_bridge/arduino_bridge.egg-info/entry_points.txt\n'}
[1.556886] (arduino_bridge) StdoutLine: {'line': b'writing requirements to ../../build/arduino_bridge/arduino_bridge.egg-info/requires.txt\n'}
[1.557096] (arduino_bridge) StdoutLine: {'line': b'writing top-level names to ../../build/arduino_bridge/arduino_bridge.egg-info/top_level.txt\n'}
[1.560928] (arduino_bridge) StdoutLine: {'line': b"reading manifest file '../../build/arduino_bridge/arduino_bridge.egg-info/SOURCES.txt'\n"}
[1.562374] (arduino_bridge) StdoutLine: {'line': b"writing manifest file '../../build/arduino_bridge/arduino_bridge.egg-info/SOURCES.txt'\n"}
[1.562754] (arduino_bridge) StdoutLine: {'line': b'running build\n'}
[1.563009] (arduino_bridge) StdoutLine: {'line': b'running build_py\n'}
[1.563272] (arduino_bridge) StdoutLine: {'line': b'running install\n'}
[1.563956] (arduino_bridge) StdoutLine: {'line': b'running install_lib\n'}
[1.566571] (arduino_bridge) StdoutLine: {'line': b'running install_data\n'}
[1.566918] (arduino_bridge) StdoutLine: {'line': b'running install_egg_info\n'}
[1.570297] (arduino_bridge) StdoutLine: {'line': b"removing '/home/koray/ros2_ws/install/arduino_bridge/lib/python3.10/site-packages/arduino_bridge-0.0.0-py3.10.egg-info' (and everything under it)\n"}
[1.570784] (arduino_bridge) StdoutLine: {'line': b'Copying ../../build/arduino_bridge/arduino_bridge.egg-info to /home/koray/ros2_ws/install/arduino_bridge/lib/python3.10/site-packages/arduino_bridge-0.0.0-py3.10.egg-info\n'}
[1.572754] (arduino_bridge) StdoutLine: {'line': b'running install_scripts\n'}
[1.607051] (arduino_bridge) StdoutLine: {'line': b'Installing arduino_bridge script to /home/koray/ros2_ws/install/arduino_bridge/lib/arduino_bridge\n'}
[1.607274] (-) TimerEvent: {}
[1.607805] (arduino_bridge) StdoutLine: {'line': b"writing list of installed files to '/home/koray/ros2_ws/build/arduino_bridge/install.log'\n"}
[1.658804] (arduino_bridge) CommandEnded: {'returncode': 0}
[1.673872] (arduino_bridge) JobEnded: {'identifier': 'arduino_bridge', 'rc': 0}
[1.676660] (-) EventReactorShutdown: {}
