[0.000000] (-) TimerEvent: {}
[0.000321] (arduino_bridge) JobQueued: {'identifier': 'arduino_bridge', 'dependencies': OrderedDict()}
[0.000578] (arduino_bridge) JobStarted: {'identifier': 'arduino_bridge'}
[0.099104] (-) TimerEvent: {}
[0.199400] (-) TimerEvent: {}
[0.299683] (-) TimerEvent: {}
[0.400046] (-) TimerEvent: {}
[0.500338] (-) TimerEvent: {}
[0.600676] (-) TimerEvent: {}
[0.700990] (-) TimerEvent: {}
[0.801304] (-) TimerEvent: {}
[0.901630] (-) TimerEvent: {}
[1.001961] (-) TimerEvent: {}
[1.011391] (arduino_bridge) Command: {'cmd': ['/usr/bin/python3', '-W', 'ignore:setup.py install is deprecated', '-W', 'ignore:easy_install command is deprecated', 'setup.py', 'egg_info', '--egg-base', 'build/arduino_bridge', 'build', '--build-base', '/home/koray/ros2_ws/arduino_bridge/build/arduino_bridge/build', 'install', '--record', '/home/koray/ros2_ws/arduino_bridge/build/arduino_bridge/install.log', '--single-version-externally-managed', 'install_data'], 'cwd': '/home/koray/ros2_ws/arduino_bridge', 'env': {'LESSOPEN': '| /usr/bin/lesspipe %s', 'MESA_LOADER_DRIVER_OVERRIDE': 'iris', 'HOSTNAME': '88d2647bf8bf', 'SHLVL': '1', 'LD_LIBRARY_PATH': '/opt/ros/humble/opt/rviz_ogre_vendor/lib:/opt/ros/humble/lib/x86_64-linux-gnu:/opt/ros/humble/lib', 'HOME': '/home/koray', 'CYCLONEDDS_URI': 'file:///etc/cyclonedds/config.xml', 'OLDPWD': '/home/koray/ros2_ws', 'ROS_PYTHON_VERSION': '3', 'ROS_DISTRO': 'humble', '_': '/usr/bin/colcon', 'ROS_VERSION': '2', 'TERM': 'xterm', 'ROS_LOCALHOST_ONLY': '0', 'PATH': '/opt/ros/humble/bin:/usr/local/sbin:/usr/local/bin:/usr/sbin:/usr/bin:/sbin:/bin', 'DISPLAY': ':0', 'LANG': 'C.UTF-8', 'RMW_IMPLEMENTATION': 'rmw_cyclonedds_cpp', 'LIBVA_DRIVER_NAME': 'i965', 'LS_COLORS': 'rs=0:di=01;34:ln=01;36:mh=00:pi=40;33:so=01;35:do=01;35:bd=40;33;01:cd=40;33;01:or=40;31;01:mi=00:su=37;41:sg=30;43:ca=30;41:tw=30;42:ow=34;42:st=37;44:ex=01;32:*.tar=01;31:*.tgz=01;31:*.arc=01;31:*.arj=01;31:*.taz=01;31:*.lha=01;31:*.lz4=01;31:*.lzh=01;31:*.lzma=01;31:*.tlz=01;31:*.txz=01;31:*.tzo=01;31:*.t7z=01;31:*.zip=01;31:*.z=01;31:*.dz=01;31:*.gz=01;31:*.lrz=01;31:*.lz=01;31:*.lzo=01;31:*.xz=01;31:*.zst=01;31:*.tzst=01;31:*.bz2=01;31:*.bz=01;31:*.tbz=01;31:*.tbz2=01;31:*.tz=01;31:*.deb=01;31:*.rpm=01;31:*.jar=01;31:*.war=01;31:*.ear=01;31:*.sar=01;31:*.rar=01;31:*.alz=01;31:*.ace=01;31:*.zoo=01;31:*.cpio=01;31:*.7z=01;31:*.rz=01;31:*.cab=01;31:*.wim=01;31:*.swm=01;31:*.dwm=01;31:*.esd=01;31:*.jpg=01;35:*.jpeg=01;35:*.mjpg=01;35:*.mjpeg=01;35:*.gif=01;35:*.bmp=01;35:*.pbm=01;35:*.pgm=01;35:*.ppm=01;35:*.tga=01;35:*.xbm=01;35:*.xpm=01;35:*.tif=01;35:*.tiff=01;35:*.png=01;35:*.svg=01;35:*.svgz=01;35:*.mng=01;35:*.pcx=01;35:*.mov=01;35:*.mpg=01;35:*.mpeg=01;35:*.m2v=01;35:*.mkv=01;35:*.webm=01;35:*.webp=01;35:*.ogm=01;35:*.mp4=01;35:*.m4v=01;35:*.mp4v=01;35:*.vob=01;35:*.qt=01;35:*.nuv=01;35:*.wmv=01;35:*.asf=01;35:*.rm=01;35:*.rmvb=01;35:*.flc=01;35:*.avi=01;35:*.fli=01;35:*.flv=01;35:*.gl=01;35:*.dl=01;35:*.xcf=01;35:*.xwd=01;35:*.yuv=01;35:*.cgm=01;35:*.emf=01;35:*.ogv=01;35:*.ogx=01;35:*.aac=00;36:*.au=00;36:*.flac=00;36:*.m4a=00;36:*.mid=00;36:*.midi=00;36:*.mka=00;36:*.mp3=00;36:*.mpc=00;36:*.ogg=00;36:*.ra=00;36:*.wav=00;36:*.oga=00;36:*.opus=00;36:*.spx=00;36:*.xspf=00;36:', 'AMENT_PREFIX_PATH': '/opt/ros/humble', 'DEBIAN_FRONTEND': 'noninteractive', 'SHELL': '/bin/bash', 'LESSCLOSE': '/usr/bin/lesspipe %s %s', 'PWD': '/home/koray/ros2_ws/arduino_bridge/build/arduino_bridge', 'QT_QPA_PLATFORM': 'xcb', 'LC_ALL': 'C.UTF-8', 'PYTHONPATH': '/home/koray/ros2_ws/arduino_bridge/build/arduino_bridge/prefix_override:/usr/lib/python3/dist-packages/colcon_core/task/python/colcon_distutils_commands:/home/koray/ros2_ws/arduino_bridge/install/arduino_bridge/lib/python3.10/site-packages:/opt/ros/humble/lib/python3.10/site-packages:/opt/ros/humble/local/lib/python3.10/dist-packages', 'COLCON': '1'}, 'shell': False}
[1.102090] (-) TimerEvent: {}
[1.202395] (-) TimerEvent: {}
[1.302691] (-) TimerEvent: {}
[1.381392] (arduino_bridge) StdoutLine: {'line': b'running egg_info\n'}
[1.382306] (arduino_bridge) StdoutLine: {'line': b'writing build/arduino_bridge/arduino_bridge.egg-info/PKG-INFO\n'}
[1.382564] (arduino_bridge) StdoutLine: {'line': b'writing dependency_links to build/arduino_bridge/arduino_bridge.egg-info/dependency_links.txt\n'}
[1.382801] (arduino_bridge) StdoutLine: {'line': b'writing entry points to build/arduino_bridge/arduino_bridge.egg-info/entry_points.txt\n'}
[1.383043] (arduino_bridge) StdoutLine: {'line': b'writing requirements to build/arduino_bridge/arduino_bridge.egg-info/requires.txt\n'}
[1.383240] (arduino_bridge) StdoutLine: {'line': b'writing top-level names to build/arduino_bridge/arduino_bridge.egg-info/top_level.txt\n'}
[1.386174] (arduino_bridge) StdoutLine: {'line': b"reading manifest file 'build/arduino_bridge/arduino_bridge.egg-info/SOURCES.txt'\n"}
[1.387218] (arduino_bridge) StdoutLine: {'line': b"writing manifest file 'build/arduino_bridge/arduino_bridge.egg-info/SOURCES.txt'\n"}
[1.387468] (arduino_bridge) StdoutLine: {'line': b'running build\n'}
[1.387582] (arduino_bridge) StdoutLine: {'line': b'running build_py\n'}
[1.387961] (arduino_bridge) StdoutLine: {'line': b'running install\n'}
[1.388750] (arduino_bridge) StdoutLine: {'line': b'running install_lib\n'}
[1.390425] (arduino_bridge) StdoutLine: {'line': b'running install_data\n'}
[1.390643] (arduino_bridge) StdoutLine: {'line': b'running install_egg_info\n'}
[1.392944] (arduino_bridge) StdoutLine: {'line': b"removing '/home/koray/ros2_ws/arduino_bridge/install/arduino_bridge/lib/python3.10/site-packages/arduino_bridge-0.0.0-py3.10.egg-info' (and everything under it)\n"}
[1.393361] (arduino_bridge) StdoutLine: {'line': b'Copying build/arduino_bridge/arduino_bridge.egg-info to /home/koray/ros2_ws/arduino_bridge/install/arduino_bridge/lib/python3.10/site-packages/arduino_bridge-0.0.0-py3.10.egg-info\n'}
[1.394708] (arduino_bridge) StdoutLine: {'line': b'running install_scripts\n'}
[1.402823] (-) TimerEvent: {}
[1.431192] (arduino_bridge) StdoutLine: {'line': b'Installing arduino_bridge script to /home/koray/ros2_ws/arduino_bridge/install/arduino_bridge/lib/arduino_bridge\n'}
[1.431700] (arduino_bridge) StdoutLine: {'line': b"writing list of installed files to '/home/koray/ros2_ws/arduino_bridge/build/arduino_bridge/install.log'\n"}
[1.471788] (arduino_bridge) CommandEnded: {'returncode': 0}
[1.488960] (arduino_bridge) JobEnded: {'identifier': 'arduino_bridge', 'rc': 0}
[1.490321] (-) EventReactorShutdown: {}
